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 Bolt List 

1996-2003

250cc

	Bag A
	
	

	Front Shock Top
	3/8”x1-1/2” 
	2

	Front Shock Bottom
	3/8”x1-1/2”
	2

	Rear Shock Top
	3/8”x1-1/2”
	2

	Rear Shock Bottom Left
	3/8”x1-3/4”
	1

	
	½” Lock Nut
	1

	
	3/8” Short Cone Spacer
	1

	Rear Shock Bottom Right
	3/8”x2”
	1

	
	½ Lock Nut
	1

	
	3/8” Long Cone Spacer
	1

	
	
	

	Bag B
	
	

	Front Radius Rod to Frame
	3/8”x1-1/4”
	3

	Front Radius Rod to Axle
	3/8”x1-1/4”
	3

	
	3/8” AN Washer
	6

	
	3/8” Lock Nut
	3

	Rear Radius Rod L&R Front
	7/16”x1-1/2” Chamfered
	2

	Rear Radius Rod RR
	7/16”x3” Chamfered
	1

	
	7/16” Long Cone Spacer
	1

	Rear Radius Rod LR
	7/16”x1-3/4”
	1

	
	7/16” Short Cone Spacer
	1

	Rear Brake Rod to Frame
	3/8”x1-3/4”
	1

	
	3/8” Lock Nut
	1

	Rear Brake Rod to Carrier
	3/8”x2”
	1

	
	3/8” Lock Nut
	1

	
	3/8” AN Washer
	2

	
	
	

	Bag C
	
	

	Panhard Bar Front
	3/8”x2-1/4”
	1

	
	3/8” Lock Nut
	2

	Tie Rod
	3/8”x2”
	2

	
	3/8” Lock Nut
	2

	
	3/8” Short Cone Spacer
	2

	Drag Link
	3/8”x2”
	1

	
	3/8” Lock Nut
	1

	
	3/8” Short Cone Spacer
	1

	Steering Arm to Spindle L-R
	5/16”x2-1/2”
	4

	
	5/16” AN Washer
	4

	*Steering Shaft*
	5/16”x5/8” Set Screw
	1

	
	5/16” Jam Nut
	1

	
	E-Clip
	1

	Steering Shaft to Drag Link
	3/8”x2-1/2”
	1

	
	3/8” Lock Nut
	1

	
	
	

	Bag D
	
	

	Master Cylinder to Frame
	5/16”x1-3/4”
	2

	
	5/16” AN Washer
	2

	Brake Caliper to Carrier
	3/8”x1-3/4”
	2

	
	3/8” Lock Nut
	2

	
	90 degree Elbow
	1

	
	
	

	Bag E
	
	

	Brake Pedal to Frame
	3/8”x2-1/2”
	1

	
	3/8” Jam Nut
	1

	Pedal to Master Cylinder
	¼”x1”
	2

	
	¼” Lock Nut
	2

	Brake Rod 4”
	¼” Jam Nut
	2

	Throttle Pedal to Frame
	3/8”x2-1/2”
	1

	
	3/8” Jam Nut
	1

	Throttle Pedal to Cable
	¼”x1”
	1

	
	¼” Lock Nut
	1

	*Throttle Rod 8”*
	¼” Jam Nut
	1

	
	Spring
	1

	
	¼” Cable Adapter
	1

	
	¼” Set Screw Collar
	1

	
	
	

	Bag F
	
	

	Bumper Bolt-Nut
	10/32”x1-1/4”
	11

	
	10/24”x1-1/2”
	1

	
	
	

	Bag G
	
	

	Wing Tree to Frame
	10/32”x1-1/4”
	2

	
	10/32” Lock Nut
	2

	Slider Shaft to Wing Tree
	5/16” Lock Nut
	2

	Cable to Slider Shaft
	10/24”x1-1/2”
	1

	
	3/16” NC Lock Nut
	1

	
	3/16” Washer
	2

	
	
	

	*Bag H*
	
	

	Fuel Tank
	3/8”x1-1/2”
	4

	
	3/8” Fender Washer
	4

	
	3/8” AN Washer
	4

	
	3/8” Lock Nut
	8

	
	3/8” O-Ring
	4

	Bracket to Frame
	3/8”x1”
	2

	
	3/8” Lock Nut
	2

	Bulk Head Fitting Assy.
	
	1

	
	¾” O-Ring
	1

	Bag I
	
	

	Birdcage Bottom
	7/16”x2-1/2”
	2

	
	7/16”x2-1/2”

Cut from 3”
	2

	
	
	

	Bag J
	
	

	Jacobs Ladder
	3/8”x1-1/2”

Cut from 2-1/4”
	1

	
	3/8”x1-3/4”

Cut from 2-1/2”
	3

	
	3/8”x3-1/2”
	1

	
	3/8” Spacer
	1

	
	3/8” Lock Nut
	1

	
	3/8” ½ Lock Nut
	4

	
	
	

	Bag K
	
	

	Chain Tensioner Arm
	3/8”x2-1/2”
	1

	
	3/8” AN Washer
	2

	
	7/16”x2-1/2”
	1

	
	7/16” Jam Nut
	1

	
	
	

	Bag L
	
	

	Torsion Stops
	5/16”x1-1/2” NC

Hex Socket Head
	4

	
	5/16” NC Jam Nut Serrated
	4

	
	5/16”x2”
	4

	
	5/16” Lock Nut Grade C
	4

	
	5/16” AN Washer
	8

	Torsion Arm Pinch
	5/16”x2”
	4

	
	5/16” Lock Nut Grade C
	4

	
	5/16” AN Washer
	8

	
	
	

	Bag M
	
	

	Shifter Arm
	3/8”x1-3/4”
	1

	
	3/8” AN Washer
	2

	
	3/8” Fender Washer
	1

	
	¼”x1-1/4”
	1

	
	¼” Lock Nut
	1

	
	¼” AN Washer
	1

	
	
	

	*Bag N*
	
	

	Seat
	3/8”x1”
	4

	
	3/8” Fender Washer
	4

	
	
	

	*Bag O*
	
	

	Air Box
	5/16”x1”
	2

	
	5/16” Lock Nut
	2

	
	5/16” Fender Washer
	2

	
	5/16”x1-1/4”
	2

	
	5/16” Lock Nut
	2

	
	5/16” AN Washer
	2

	
	Rubber Spacer
	2

	
	
	

	*Bag P*
	
	

	
	Dzus Buttons
	27

	
	Dzus Springs
	27

	
	Dzus Rivets 1/8”x3/16” Grip
	54


*Optional*


