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Bolt List for Deluxe Kit

2013
600cc

All Bolts are National Fine unless stated

	Bag A

	Front Shock Top
	3/8”x1-1/4”
	2

	Front Shock Bottom
	3/8”x1-1/4”
	2

	Rear Shock Top
	3/8”x1-1/4”
	2

	Rear Shock Bottom Left
	3/8”x1-1/2”
	1

	
	3/8” ½ Lock Nut
	1

	
	3/8” AN Washer
	2

	Rear Shock Bottom Right
	3/8”x2-1/2”
	1

	
	3/8” ½ Lock Nut
	1

	Bag B

	Front Radius Rod to Frame
	3/8”x1-1/4”
	3

	Front Radius Rod to Axle
	3/8”x1”
	3

	
	3/8” ½ Lock Nut
	3

	Rear Radius Rod R Front
	7/16”x1-1/4” Chamfered
	1

	Rear Radius Rod L Front
	7/16”x2-3/4”Chamfered
	1

	
	7/16” ½ Lock Nut
	1

	Rear Brake Rod to Frame
	7/16”x3” 
	1

	
	7/16” ½ Lock Nut
	1

	Bag C

	Panhard Bar Front
	3/8”x2-1/4”
	1

	
	3/8” ½ Lock Nut
	2

	Tie Rod
	3/8”x3”
	1

	
	3/8”x2”
	1

	
	3/8” ½ Lock Nut
	2

	Rack & Pinion
	5/16”x3”
	2

	
	5/16” ½ Lock Nut
	2

	Rack & Pinion to Drag Link
	3/8”x2 1/2”
	1

	
	**2-1/4” w/ Chromalloy tab

3/8” Lock Nut
	1

	Upper Steering Bracket to Frame
	5/16”x1-3/4”
	2

	
	5/16” ½ Lock Nut
	2

	Steering Arm to Spindle
	3/8” x1-1/4”
	4

	
	3/8” AN Washer
	4

	Bag E

	Master Cylinder to Frame
	5/16”x1-1/2”
	2

	
	5/16” ½ Lock Nut
	2

	Brake Pedal to Frame
	3/8”x3”

3/8” AN Washer
	1

1

	
	3/8” Jam Nut
	1

	Pedal to Master Cylinder
	¼”x3/4”
	1

	
	¼” ½ Lock Nut
	1

	Throttle Pedal to Frame
	3/8”x2-1/4”
	1

	
	3/8” Jam Nut
	1

	Throttle Pedal to Rod
	¼”x1-1/4”
	1

	
	¼” AN Washer
	1

	
	¼” Lock Nut
	1

	Bell Crank to Frame
	¼” x 1” 
	1

	
	¼” AN Washer
	2

	
	¼” Jam Nut
	2

	
	¼” x 1”
	1

	Bell Crank to Rod End


	¼” Lock Nut
	1

	
	¼” AN Washer
	1

	Bag F

	Bumper/Nerfs Bars
	10/32”x1-1/4”
	14

	
	3/16” Lock Nut
	14

	Bag G

	Rear Wing Tree to Frame
	5/16”x1-1/4”
	2

	
	5/16” ½ Lock Nut
	2

	Front Wing Tree to Frame

“Pinch Style”
	¼”x1-1/4”
	2

	
	¼”-½ Lock Nut
	2

	Nose Wing Post to Frame
	¼”x1-1/4”
	2

	
	¼”-½ Lock Nut
	2

	Rear Tree to Wing
	5/16”x1-3/4”
	1

	
	5/16” ½ Lock Nut
	1

	
	5/16”x2-1/2”
	1

	
	5/16” Lock Nut
	1

	Slider Tube to Frame
	5/16”x1-1/2”
	1

	
	5/16” ½ Lock Nut
	1

	Nose Wing Panel Mounts
	¼” AN Washer
	8

	
	¼” x ¾” 
	2

	
	¼” -½ Lock Nut
	2

	*Bag H*

	Fuel Tank – Wet Tank
	3/8”x1”
	4

	
	3/8” ½ Lock Nut
	4

	
	3/8” AN Washer
	4

	
	3/8” USS GR9 Washer
	4

	
	3/8” Stat-O-Seal (Box)
	2

	Fuel Tank – Bladder Tank
	5/16”x3/4” NC Socket Head
	4

	
	5/16” Lock Washer
	4

	Bag J

	Jacobs Ladder
	3/8”x1-1/2”

Cut from 2-1/4”
	1

	
	3/8”x1-3/4”

Cut from 2-1/2”
	4

	
	3/8” ½ Lock Nut
	5

	
	3/8” AN Washer
	9

	Bag M

	Shifter Arm
	3/8”x1-1/2” Countersunk Socket Head
	1

	
	3/8” Jam nut
	1

	
	¼”x1-1/4”
	1

	
	¼” AN Washer
	1

	
	¼” ½ Lock Nut  
	1

	Bag R



	Steering Wheel to Hub
	5/16”x3/4” NC Hex Socket Head Plated
	3

	
	5/16” AN Washer
	3



