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Bolt List 

1998-2004

600cc

All Bolts are National Fine unless stated

	Bag A
	
	

	Front Shock Top
	3/8”x1-1/4” (1-1/2” Coil)
	2

	Front Shock Bottom
	3/8”x1-1/4” (1-1/2” Coil)
	2

	Rear Shock Top
	3/8”x1-1/4”
	2

	Rear Shock Bottom Left
	3/8”x1-3/4”
	1

	
	3/8” ½ Lock Nut
	1

	
	3/8” Short Cone Spacer*
	1

	
	*For 2004 use 3/8” AN Washer
	2

	Rear Shock Bottom Right
	3/8”x2-1/2”
	1

	
	3/8” ½ Lock Nut
	1

	
	3/8” Long Cone Spacer
	1

	
	Shock Reducer Bushings
	8

	
	
	

	Bag B
	
	

	Front Radius Rod to Frame
	3/8”x1-1/4”
	3

	Front Radius Rod to Axle
	3/8”x1-1/4”
	3

	
	3/8” AN Washer*
*99-03 Only
	6

	
	3/8” ½ Lock Nut
	3

	Rear Radius Rod R Front
	7/16”x1-1/4” Chamfered
	1

	Rear Radius Rod L Front
	7/16”x2-1/2” Chamfered
	1

	
	7/16”x2-3/4 Chamfered *03+
	1

	
	7/16” ½ Lock Nut
	1

	Rear Brake Rod to Frame
	7/16”x2-1/2” Chamfered
	1

	
	7/16”x2-3/4 Chamfered *03+
	1

	
	7/16” ½ Lock Nut
	1

	Rear Radius Rod RR
	7/16”x1-1/2” Chamfered
	1

	
	7/16”x1-1/4” Chamfered *03+
	1

	
	7/16” Long Cone Spacer*
*99-03 Only
	1

	Rear Radius Rod LR
	7/16”x1-1/4” Chamfered
	1

	
	7/16” Short Cone Spacer*
*99-03 Only
	1

	Rear Brake Rod to Carrier
	7/16”x1-1/4”
	1

	
	
	

	Bag C
	
	

	Panhard Bar Front
	3/8”x2-1/4”
	1

	
	3/8” ½ Lock Nut
	2

	Tie Rod
	3/8”x2-3/4” LS*

*3” for 2004
	1

	
	3/8”x1-3/4” RS
	1

	
	3/8” ½ Lock Nut
	2

	
	3/8” Short Cone Spacer
	2

	Drag Link
	3/8” Long Cone Spacer
	1

	Steering Arm to Spindle L-R
	5/16”x1-3/4” NC

Hex Socket Head Plated
	4

	Steering Shaft
U-Joints
	5/16”x1-1/2”
	4

	
	5/16” AN Washer
	8

	
	5/16” Lock Nut
	4

	Rack & Pinion
	5/16”x3”
	2

	
	5/16” ½ Lock Nut
	2

	Rack & Pinion to Drag Link
	3/8”x2-1/4”
	1

	
	3/8” Lock Nut
	1

	
	3/8” Tapered Spacer
	1

	Upper Steering Bracket to Frame
	5/16”x1-3/4”
	2

	
	5/16” ½ Lock nut
	2

	
	
	

	*Bag D*
	
	

	Brake Caliper to Carrier
	3/8”x1-1/2” NF

Hex Socket Head Plated
	2

	
	3/8” ½ Lock Nut
	2

	
	90 degree Elbow
	1

	
	
	

	Bag E
	
	

	Master Cylinder to Frame
	5/16”x1-1/2”
	2

	
	5/16” ½ Lock Nut
	2

	Brake Pedal to Frame
	3/8”x2-3/4”
	1

	
	3/8” ½ Lock Nut
	1

	Pedal to Master Cylinder
	¼”x1”
	2

	
	¼” Lock Nut
	2

	*Brake Rod 4”*
	¼” Jam Nut
	2

	Throttle Pedal to Frame
	3/8”x2-1/4”
	1

	
	3/8” Jam Nut
	1

	Throttle Pedal to Cable
	¼”x1”
	1

	
	¼” Lock Nut
	1

	
	¼” AN Washer
	1

	*Throttle Rod 8”*
	¼” Jam Nut
	1

	
	Spring
	1

	
	¼” Cable Adapter
	1

	
	¼” Set Screw Collar
	1

	
	
	

	Bag F
	
	

	Bumper Bolt-Full Lock Nut
	10/32”x1-1/4”
	14

	
	
	

	Bag G
	
	

	Rear Wing Tree to Frame
	5/16”x1-1/4”
	2

	
	5/16” ½ Lock Nut
	2

	Front Wing Tree to Frame

“Pinch Style”
	¼”x1-1/4”
	2

	
	¼”-½ Lock Nut
	2

	Nose Wing Post to Frame
	¼”x1-1/4”
	2

	
	¼”-½ Lock Nut
	2

	Rear Tree to Wing
	5/16”x1-3/4”
	1

	
	5/16” ½ Lock Nut
	1

	
	5/16”x2-3/4”
	1

	
	5/16” ½ Lock Nut
	1

	Cable to Slider Shaft
	10/24”x1-1/2”
	1

	
	3/16” NC Lock Nut
	1

	Slider Tube to Frame
	5/16”x1-1/2”
	1

	
	5/16” ½ Lock Nut
	1

	
	
	

	*Bag H*
	
	

	Fuel Tank
	3/8”x1-1/2”
	4

	
	3/8” Fender Washer
	4

	
	3/8” AN Washer
	4

	
	3/8” ½ Lock Nut
	6

	
	3/8” Lock Nut
	2

	
	3/8” O-Ring
	4

	Bulk Head Fitting Assy.
	
	1

	
	¾” O-Ring
	1

	*For 2004
	5/16”x3/4”NC Socket Head
	4

	
	5/16” Lock Washer
	4

	
	
	

	Bag I
	
	

	Birdcage Bottom
	7/16”x2-1/2”
	2

	
	7/16”x2-1/2”

Cut from 3”
	2

	
	*Cut from 2-3/4 for 04
(1/ea for 2004)
	

	
	
	

	Bag J
	
	

	Jacobs Ladder
	3/8”x1-1/2”

Cut from 2-1/4”
	1

	
	3/8”x1-3/4”

Cut from 2-1/2”
	4

	
	3/8”x3-1/2”
	1

	
	7/8” Spacer
	1

	
	3/8” Lock Nut
	1

	
	3/8” ½ Lock Nut
	5

	
	3/8” AN Washer
	7

	
	
	

	Bag L

(Double for 4-Bar Car)
	
	

	Torsion Stops


	5/16”x1-1/2” NC

Hex Socket Head
	2

	
	5/16” NC Jam Nut Serrated
	2

	
	5/16”x2”
	2

	
	5/16” Lock Nut Grade C
	2

	
	5/16” AN Washer
	4

	Torsion Arm Pinch
	5/16”x2”
	2

	
	5/16” Lock Nut Grade C
	2

	
	5/16” AN Washer
	4

	
	
	

	Bag M
	
	

	Shifter Arm
	3/8”x1-3/4”
	1

	
	3/8” Jam Nut
	1

	
	¼”x1-3/4”
	1

	
	¼” Lock Nut
	1

	For 2004
	3/8”x1-1/2” Countersunk Socket Head
	1

	
	3/8” Full Nut
	1

	
	¼”x1-1/4”
	1

	
	¼” AN Washer
	1

	
	¼” ½ Lock Nut  
	1

	
	
	

	*Bag P*
	
	

	
	Dzus Buttons
	

	
	Dzus Springs
	

	
	Dzus Rivets 1/8”x3/16” Grip
	

	
	
	

	Bag Q
	
	

	Brake Carrier
	¼”x1”

Hex Socket Head Plated
	6

	
	¼” AN Washer
	12

	
	¼” Lock Nut
	6

	Sprocket Carrier
	5/16”x1” NC

Hex Socket Head Plated
	6

	
	5/16” NC Serrated Flange Nut
	6


*Optional*


